AIRMAN  
Aeronautics  
Airman XB-70 Pro Flight Computer

Product Development Workflow

XB-70 Pro Flight controller hardware components:

Main Processor : STM32H747XIH6 (32-bit Arm® Cortex®-M7 and 32-bit Arm® Cortex®-M4 480MHz)

BMI360 : Programmable smart sensor combining accelerometer, gyroscope and fusion software.

BMM355 : 3-axis magnetic sensor with high data rate.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
| SHT41-AD1F-R2 | Sensirion_SHT4x-AD1F |  |  |